set_property IOSTANDARD LVCMOS33 [get_ports {data1[3]}]
set_property IOSTANDARD LVCMOS33 [get_ports {data1[2]}]
set_property IOSTANDARD LVCMOS33 [get_ports {data1[1]}]
set_property IOSTANDARD LVCMOS33 [get_ports {data1[0]}]
set_property IOSTANDARD LVCMOS33 [get_ports {data2[3]}]
set_property IOSTANDARD LVCMOS33 [get_ports {data2[2]}]
set_property IOSTANDARD LVCMOS33 [get_ports {data2[1]}]
set_property IOSTANDARD LVCMOS33 [get_ports {data2[0]}]
set_property IOSTANDARD LVCMOS33 [get_ports {result[4]}]
set_property IOSTANDARD LVCMOS33 [get_ports {result[3]}]
set_property IOSTANDARD LVCMOS33 [get_ports {result[2]}]
set_property IOSTANDARD LVCMOS33 [get_ports {result[1]}]
set_property IOSTANDARD LVCMOS33 [get_ports {result[0]}]
set_property IOSTANDARD LVCMOS33 [get_ports {seg[6]}]
set_property IOSTANDARD LVCMOS33 [get_ports {seg[5]}]
set_property IOSTANDARD LVCMOS33 [get_ports {seg[4]}]
set_property IOSTANDARD LVCMOS33 [get_ports {seg[3]}]
set_property IOSTANDARD LVCMOS33 [get_ports {seg[2]}]
set_property IOSTANDARD LVCMOS33 [get_ports {seg[1]}]
set_property IOSTANDARD LVCMOS33 [get_ports {seg[0]}]
set_property IOSTANDARD LVCMOS33 [get_ports {seg_cs[3]}]
set_property IOSTANDARD LVCMOS33 [get_ports {seg_cs[2]}]
set_property IOSTANDARD LVCMOS33 [get_ports {seg_cs[1]}]
set_property IOSTANDARD LVCMOS33 [get_ports {seg_cs[0]}]
set_property IOSTANDARD LVCMOS33 [get_ports {type[4]}]
set_property IOSTANDARD LVCMOS33 [get_ports {type[3]}]
set_property IOSTANDARD LVCMOS33 [get_ports {type[2]}]
set_property IOSTANDARD LVCMOS33 [get_ports {type[1]}]
set_property IOSTANDARD LVCMOS33 [get_ports {type[0]}]
set_property PACKAGE_PIN P5 [get_ports {data1[3]}]
set_property PACKAGE_PIN P4 [get_ports {data1[2]}]
set_property PACKAGE_PIN P3 [get_ports {data1[1]}]
set_property PACKAGE_PIN P2 [get_ports {data1[0]}]
set_property PACKAGE_PIN R2 [get_ports {data2[3]}]
set_property PACKAGE_PIN M4 [get_ports {data2[2]}]
set_property PACKAGE_PIN N4 [get_ports {data2[1]}]
set_property PACKAGE_PIN R1 [get_ports {data2[0]}]
set_property PACKAGE_PIN F6 [get_ports {result[4]}]
set_property PACKAGE_PIN G4 [get_ports {result[3]}]
set_property PACKAGE_PIN G3 [get_ports {result[2]}]
set_property PACKAGE_PIN J4 [get_ports {result[1]}]
set_property PACKAGE_PIN H4 [get_ports {result[0]}]
set_property PACKAGE_PIN D4 [get_ports {seg[6]}]
set_property PACKAGE_PIN E3 [get_ports {seg[5]}]
set_property PACKAGE_PIN D3 [get_ports {seg[4]}]
set_property PACKAGE_PIN F4 [get_ports {seg[3]}]
set_property PACKAGE_PIN F3 [get_ports {seg[2]}]
set_property PACKAGE_PIN E2 [get_ports {seg[1]}]
set_property PACKAGE_PIN D2 [get_ports {seg[0]}]
set_property PACKAGE_PIN G1 [get_ports {seg_cs[3]}]
set_property PACKAGE_PIN F1 [get_ports {seg_cs[2]}]
set_property PACKAGE_PIN E1 [get_ports {seg_cs[1]}]
set_property PACKAGE_PIN G6 [get_ports {seg_cs[0]}]
set_property PACKAGE_PIN U4 [get_ports {type[4]}]
set_property PACKAGE_PIN V1 [get_ports {type[3]}]
set_property PACKAGE_PIN R15 [get_ports {type[2]}]
set_property PACKAGE_PIN R11 [get_ports {type[1]}]
set_property PACKAGE_PIN R17 [get_ports {type[0]}]

set_property PACKAGE_PIN P17 [get_ports clk]
set_property IOSTANDARD LVCMOS33 [get_ports clk]
