set_property IOSTANDARD LVCMOS33 [get_ports {seg1[6]}]
set_property IOSTANDARD LVCMOS33 [get_ports {seg1[5]}]
set_property IOSTANDARD LVCMOS33 [get_ports {seg1[4]}]
set_property IOSTANDARD LVCMOS33 [get_ports {seg1[3]}]
set_property IOSTANDARD LVCMOS33 [get_ports {seg1[2]}]
set_property IOSTANDARD LVCMOS33 [get_ports {seg1[1]}]
set_property IOSTANDARD LVCMOS33 [get_ports {seg1[0]}]
set_property IOSTANDARD LVCMOS33 [get_ports {seg2[6]}]
set_property IOSTANDARD LVCMOS33 [get_ports {seg2[5]}]
set_property IOSTANDARD LVCMOS33 [get_ports {seg2[4]}]
set_property IOSTANDARD LVCMOS33 [get_ports {seg2[3]}]
set_property IOSTANDARD LVCMOS33 [get_ports {seg2[2]}]
set_property IOSTANDARD LVCMOS33 [get_ports {seg2[1]}]
set_property IOSTANDARD LVCMOS33 [get_ports {seg2[0]}]
set_property PACKAGE_PIN B4 [get_ports {seg1[6]}]
set_property PACKAGE_PIN A4 [get_ports {seg1[5]}]
set_property PACKAGE_PIN A3 [get_ports {seg1[4]}]
set_property PACKAGE_PIN B1 [get_ports {seg1[3]}]
set_property PACKAGE_PIN A1 [get_ports {seg1[2]}]
set_property PACKAGE_PIN B3 [get_ports {seg1[1]}]
set_property PACKAGE_PIN B2 [get_ports {seg1[0]}]
set_property PACKAGE_PIN D4 [get_ports {seg2[6]}]
set_property PACKAGE_PIN E3 [get_ports {seg2[5]}]
set_property PACKAGE_PIN D3 [get_ports {seg2[4]}]
set_property PACKAGE_PIN F4 [get_ports {seg2[3]}]
set_property PACKAGE_PIN F3 [get_ports {seg2[2]}]
set_property PACKAGE_PIN E2 [get_ports {seg2[1]}]
set_property PACKAGE_PIN D2 [get_ports {seg2[0]}]

set_property IOSTANDARD LVCMOS33 [get_ports {seg_cs1[3]}]
set_property IOSTANDARD LVCMOS33 [get_ports {seg_cs1[2]}]
set_property IOSTANDARD LVCMOS33 [get_ports {seg_cs1[1]}]
set_property IOSTANDARD LVCMOS33 [get_ports {seg_cs1[0]}]
set_property IOSTANDARD LVCMOS33 [get_ports {seg_cs2[3]}]
set_property IOSTANDARD LVCMOS33 [get_ports {seg_cs2[2]}]
set_property IOSTANDARD LVCMOS33 [get_ports {seg_cs2[1]}]
set_property IOSTANDARD LVCMOS33 [get_ports {seg_cs2[0]}]
set_property PACKAGE_PIN G2 [get_ports {seg_cs1[3]}]
set_property PACKAGE_PIN C2 [get_ports {seg_cs1[2]}]
set_property PACKAGE_PIN C1 [get_ports {seg_cs1[1]}]
set_property PACKAGE_PIN H1 [get_ports {seg_cs1[0]}]
set_property PACKAGE_PIN G1 [get_ports {seg_cs2[3]}]
set_property PACKAGE_PIN F1 [get_ports {seg_cs2[2]}]
set_property PACKAGE_PIN E1 [get_ports {seg_cs2[1]}]
set_property PACKAGE_PIN G6 [get_ports {seg_cs2[0]}]

set_property IOSTANDARD LVCMOS33 [get_ports {votes[4]}]
set_property IOSTANDARD LVCMOS33 [get_ports {votes[3]}]
set_property IOSTANDARD LVCMOS33 [get_ports {votes[2]}]
set_property IOSTANDARD LVCMOS33 [get_ports {votes[1]}]
set_property IOSTANDARD LVCMOS33 [get_ports {votes[0]}]
set_property PACKAGE_PIN P5 [get_ports {votes[4]}]
set_property PACKAGE_PIN P4 [get_ports {votes[3]}]
set_property PACKAGE_PIN P3 [get_ports {votes[2]}]
set_property PACKAGE_PIN P2 [get_ports {votes[1]}]
set_property PACKAGE_PIN R2 [get_ports {votes[0]}]
