set_property IOSTANDARD LVCMOS33 [get_ports clk]
set_property IOSTANDARD LVCMOS33 [get_ports clk_1Hz]
set_property IOSTANDARD LVCMOS33 [get_ports clk_12Hz]
set_property IOSTANDARD LVCMOS33 [get_ports clk_48Hz]
set_property IOSTANDARD LVCMOS33 [get_ports clk_190Hz]
set_property IOSTANDARD LVCMOS33 [get_ports reset]
set_property PACKAGE_PIN P17 [get_ports clk]
set_property PACKAGE_PIN R1 [get_ports reset]
set_property PACKAGE_PIN G3 [get_ports clk_1Hz]
set_property PACKAGE_PIN J4 [get_ports clk_12Hz]
set_property PACKAGE_PIN H4 [get_ports clk_48Hz]
set_property PACKAGE_PIN J3 [get_ports clk_190Hz]

